<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">       Printer definition file for WSSINDEX custom print utility

All lines of this file are comments until a line beginning ----.  After that,
alternate lines are comments and parameters.  See the CUSTPRNT documentation
for a description of the format allowed here.  The codes in the distributed
version of this file are for an Epson-compatible dot matrix printer, but you
may alter these to suit your needs.  To make it easier for people to read the
printer sequences, I have used blanks to separate characters, and commas to
separate multi-character printer commands.  Most of these delimiters are
not required by the routine which reads this file.

Canon LBP-8A1 commands should work with LBP-8A2 and probably other Canon
laser printers.

Commands used in this file:

  \e ; = go to ISO mode
  \e &lt; = soft reset
  \e [ \2 \s K = 15 character per inch
  \e [ \4 \s L = 8 lines per inch
  \n \e [ \2 t = advance one line then set top margin to current position
  \f = form feed
  \e : = go to Diablo mode

------------------------------------------------------------
Printer name
Canon LBP-8A1 laser printer, ISO mode
Optional string printed on all labels
Property of &lt;your name here&gt;
Printer initialization command for 1,2,... column printing, 50 max
\e ;,\e &lt;,\e [ \2 \s K,\e [ \4 \s L,\n,\e [ \2 t
Printer initialization command for labels, 50 max (pitch, line spacing, etc.)

Printer initialization command for disk covers, 50 max

Printer deinitialization command, 10 max (form feed for laser printer, etc.)
\f,\e :
Number of spaces in left margin for labels
5
Number of columns for labels
1
Width of labels (characters)
50
Number of characters between labels (if multiple columns)
5
Length of label in lines (including unusable lines)
12
Number of usable lines for label
9
Number of spaces in left margin for disk covers
0
Width of paper for disk covers (characters)
90
Length of page in lines for disk covers
40
Printer command to position for the next disk cover
10 10 10 10
Character to use for sides of disk cover box (32 = blank prints faster)
245
Character to use for top and bottom lines
241
Character to use for top left corner
240
Character to use for top right corner
242
Character to use for bottom left corner
246
Character to use for bottom right corner
247
End of printer configuration file
</pre></body></html>